|  |  |  |
| --- | --- | --- |
| **SERVICE** | **SEPTEMBER** | **MARCH** |
| BATTERY CONNECTIONS; CLEAN IF NECESSARY |  |  |
| BODY AND DOOR DRAIN HOLES FOR OBSTRUCTIONS; CLEAN IF NECESSARY |  |  |
| COOLING SYSTEM FLUID LEVEL AND COOLANT STRENGTH |  |  |
| DOOR WEATHERSTRIPS FOR WEAR; LUBRICATE IF NECESSARY |  |  |
| HINGES/LATCHES/OUTSIDE LOCKS FOR PROPER OPERATION; LUBRICATE IF NECESSARY |  |  |
| PARKING BRAKE FOR PROPER OPERATION |  |  |
| SAFETY BELTS AND SEAT LATCHES FOR WEAR AND FUNCTION  |  |  |
| SAFETY WARNING LAMPS (BRAKE, ABS, AIR BAG, SAFETY BELT) FOR OPERATION |  |  |
| WASHER SPRAY/WIPER OPERATION; CLEAN AND REPLACE BLADES AS NECESSARY |  |  |
| INSPECTION PERFORMED BY: | NAME:DATE: | NAME:DATE: |